**Products list**

***To hand-made products of Fosa-dog company***

*(part of terms & conditions* [*www.fosa-dog,com/en*](http://www.fosa-dog,com/en) *)*

**Materials:**

* ***Nylon***
  + Polypropylene (PP) strap, the most common single strap thickness is 1.5 mm, then 1.2 or 1 mm according to the manufacturer or available colors.
* ***Ribbon***
  + *Grosgrain* ***r****ibbons* with available pattern and in various widths. Material polyester.
  + *Printed ribbons* with available pattern and in various widths. Ribbon printing is disturbed both mechanically and due to different temperatures or moisture.
* ***Belt buckle***
  + *Metal - polished steel (PO)* - stainless steel (SS), load limit 400 kg (width 2,5cm), 330 kg (width 3 cm and 4 cm) and 500 kg (width 5cm).
  + *Metal - black* - steel (ST), surface treatment matt black (BK) (impact toughness, color is easily scrabed by sharp objects and no resistance to metal - metal contact). Load capacity 200 kg (width 2,5 cm) and 300 kg (width 3 cm and 4 cm).
  + *Buckle with two spines* - 5cm - steel (ST), chrome-plated (CT), maximum load 450 kg.
* ***Trident***
  + *Plastic 2.5 cm* - acetal (POM) material. Breaking load 55 kg.
  + *Metal - Zinc alloy* (ZDC), nickel (NP). 200kg breaking load.
  + *Metal - black* - material zinc alloy (ZDC), surface treatment matt black (BK) (impact toughness, color is easily scrabed by sharp objects and no resistance to metal - metal contact). 200kg breaking load.
* ***Snap-hook***
  + *Chromium* - Zinc alloy (ZDC), chrome (CP). Breaking load from 150 to 250kg depending on size.
  + *Black* - Zinc alloy (ZDC), surface treatment matt black (BK) (impact toughness, color is easily scrabed by sharp objects and no resistance to metal - metal contact). Breaking load from 150 to 250kg depending on size.
* **D-ring**
  + *Stainless* - stainless steel (SS), polished steel (PO). Solid welded joint. Breaking load 250kg (2.5 width), 350kg (3cm and 4cm width) and 390kg (5cm width).
  + *Black* - steel (ST), surface treatment matt black (BK) (impact toughness, color is easily scrabed by sharp objects and no resistance to metal - metal contact). Solid welded joint. Breaking load 220kg (2.5cm width), 270kg (3cm width), 300kg (4cm and 5cm width).
* **Ring**
  + *Stainless* - stainless steel (SS), polished steel (PO). Solid welded joint. Breaking load 150 - 300kg depending on size.
  + *Black* - steel (ST), surface treatment matt black (BK) (impact toughness, color is easily scrabed by sharp objects and no resistance to metal - metal contact). Solid welded joint. Breaking load 200kg - 300kg depending on size
* **Grommets**
  + *Collars in width 2,5 and 3 cm* - material stainless steel (SS), finish polished steel (PO).
  + *Collars 4 and 5 cm* - material steel (ST), surface treatment nickel (NP).
  + *Black grommets (all widths)* - material steel (ST), surface treatment old copper (AC).
* **Rivets**
  + *Nickel* - material steel (ST), surface treatment nickel (NP).
  + *Black* - material steel (ST), surface treatment copper (AC).
* **Threads**
  + *Jeans threads* – material 100% polyester, thread thickness 0,5mm, tex 30x3, high strength.

**Údržba:**

* **Products – just from nylon**
  + Machine washable up to 40 ° C without bleaching or other aggressive cleaning agents.
  + Do not clean chemically.
  + Do not dry in the dryer.
  + Do not iron.
* **Products – nylon + ribbon**
  + It is recommended not to wash in an automatic washing machine.
  + Handle with care when wet.
  + Do not use bleach or other aggressive cleaners.
  + Do not clean chemically.
  + Do not iron.
  + Do not dry in the dcer.
* When washing in an automatic washing machine, we recommend wrapping the metal parts of the products (buckles, snap-hooks, tridents, etc.) in a cloth (eg sock, elastic bandage, bandage) to protect both the washing machine and the metal parts of the product.
* Although our products are intended for animals, it is recommended not to expose them to moisture and wet for a long time. If this happens (walking in the rain, outdoor bathing, etc.), please let the product dry in the sun or at home in a dry place.
* Metal parts of the product that are not made of stainless steel may be subject to corrosion.
* Please remember that the nylons and ribbons of which our products are made were not made purely for use in the everyday life of a "four-legged" family member ☺ But we still hope for their long lifetime ☺

*Team* ***Fosa-dog***